W 1000 WATT
POWER INVERTER
Instruction Manual
IMPORTANT: READ AND UNDERSTAND ALL WARNINGS AND INSTRUCTIONS INCLUDED IN INSTRUCTION MANUAL PRIOR TO USE.
Two Standard
220V AC Outlets	High-Speed
ON/OFF Rocker Switch	Cooling Fan	Positive Power Input Terminal
LED Indicator Light	Negative Power Input Terminal (Green=Power ON.. Orange =Protection mode)
Front Panel
 
Rear Panel
WARNING: This inverter must be connected only to a 12 volt DC Negative Ground ignition system. Most vehicles are negative ground systems. Do not use this inverter with Positive Ground vehicle ignition systems. Consult your vehicle owner's manual for ignition system identification.
POWER SOURCE
This inverter must be connected to a 12 volt DC negative ground ignition system battery in good condition. Most vehicles are negative ground systems(See vehicle owner's manual for ignition system identification).
CAUTION:
* Do not connect this inverter to a 6 volt or 24 volt DC battery system.
* Do not use this inverter with Positive Ground vehicle to avoid damage to the inverter.

1. DETERMINE POWER REQUIREMENT:
To determine maximum power required, add up the wattage of all devices to be operated with this inverter simultaneously. If the wattage of devices is not available, but the current draw (amp) is given, simply convert to wattage using this formula:
Volts(V)xAmps(A)=watts(W)
EXAMPLE:220 volts x 2 amps =440 watts.
2.OPERATING INSTRUCTIONS:
NOTE:If power requirements exceeds 1000 watts, DO NOT plug directly to vehicle accessory socket.This inverter must then be connected directly to battery using the Battery Terminal Adaptor Kit provided. For 1000 watts or less go to step A For device(s) with over 1000 watts go to step B.

A.Accessorv Plug Connection:
Prior to connecting inverter, make sure the inverter ON/OFF rocker switch is in the OFF position.
B. Battery Terminal Kit Use:
I. Prior to connecting inverter, make sure the inverter ON/OFF rocker switch is in the OFF position. 2.Connect the BLACK alligator clip to the NEGATIVE(-)terntinal of vehicle battery and connect the RED alligator clip to the POSITIVE(+)terminal of vehicle battery.
C. PLUGGING IN DEVICE(S):

•	SYSTEM NORMAL OPERATION 	GPEEN LED INDICATOR
•	OVER TEMPERATURE 	RED LED INDICATOR
•	OVERLOAD 	RED LED INDICATOR
•	LOW/HIGH BATTERY 	RED LED INDICATOR
I. Prior to plugging in device(s), make sure the devices(s) is OFF.
2.Connect the device(s) electrical plug into the inverter receptacle(s).
3.Turn the inverter ON/OFF switch, to ON position. If the inverter is working properly a green LED indicator on the front panel will light.Then trun ON the device(s). If the green indicator remains ON, then the system is operating properly. If inverter alarm sounds or the red LED indicator light turns on, turn OFF the device(s) then turn OFF the inverter immediately. See the trouble shooting guide. The inverter may have been over loaded or the input voltage may be too low.

CAUTION: Some rechargeable devices are equipped with a separate charger, which can be connected into this inverters AC receptacle(s). The inverters are engineered to be used with these products. However, certain rechargeable devices are manufactured with built-in chargers (See device owner's manual). This category of devices may cause internal damage to inverters and should not be used with this inverter. The temperature of device(s) must be monitored for first 15 minutes of operation. Abnormally elevated temperature of device(s) ism indication that they should not be used with this inverter.
TYPICAL USE AND WATTAGE
NOTE:
To convert amps to wattage use this formula: Volts x Amps=Watts
This listing is for reference purposes only. Some devices exceed the wattages listed Before using device refer to device owner's manual for actual wattage required
BATTERY TERMINAL ADAPTOR SOCKET Connect these terminals to the color coded _terminals on the back panel of the inverter -"

 
Connect these terminals to the color coded cable clamps to your battery terminals (Red-positive, Black-negative)
1000WATT INVERTER
VEHICLE BATTERY
Soldering gun 135 watts Glue gun 20 watts 114 hp Power Buffer 110 watts Cordless Drill Charger(7volts)	15 watts
 
Laptop computer	90 watts
Fax machine	170 watts
 
13 "color T. V. 70 watts 20"color T.V./VCR combo 120 watts 27"color T.V. 160 watts VCR 45 watts CD changer	65 watts
01
Cellular phone Charger 30 watts Camcorder Charger(6 volts) 25 watts Air Compressor Charger	90 watts
-2
-3-
WARNINGS
-Read and understand all operating instructions in this manual prior to operating this inverter to avoid damage to inverter, power source or device connected to the inverter. *Improper use of this inverter can cause personal injury, porperty damage, and or loss of life .
•	his inverter must be connected only to a 12 volt DC Negative Ground ignition system(most vehicles). Do not use this inverter with Positive Ground vehicle ignition system.Consult your vehicle owner's manual for ignition system identification.
*Do not use this inverter with device(s) which use more than 1000 watts power consumption.Make certain the wattage requirements are within the capacity of this inverter output watts range. *Do not connect inverter to household or RV. AC distributing circuit. Do not connect inverter to AC load circuit in which the neutral wire is connected to ground(-)or to negative of the DC battery power source.
*Do not connect to a 6 volt or 24 volt DC battery.
-Do not exceed the maximum input voltage of 15 volt DC (direct current).
-Do not use or place this inverter near flammable materials or any location which accumulate flammable fumes.
-Do not operate this inverter in or near water. Do not operate inverter using wet hands.
-Do not touch the tip of the inverter cigarette lighter plug immediately after usage.The plug may be hot and could cause minor burns.
-Do not allow the inverter's cord or any operating device's cord to restrict driving. -Disconnect power to the inverter when it is not in use.
*This is not a toy. Keep away from reach of children.
•	o avoid potential property damage, do not leave this inverter or any device operating unattended in vehicle.

CAUTIONS
•	o not place this inverter in confined spaces or inside battery compartment of vehicle or boat. Use only in properly ventilated areas.
•	o not place item(s) over the inverter. Make sure that air is allowed to circulate freely around it. -Do not place the inverter in direct sunlight or near any device which is generating heat above room tempeature.
-Do not operate inverter in ambient air temperature below 32 - F or above 95 , F. -Do not open the inverter housing case.
-Secure the inverter and device(s) being operated to prevent them from moving while the vehicle is in motion.
-Do not use an AC(220 volt) extention cord longer than 25 feet.
-Do not use a 12 volt DC extension cord of any type or length.
*Start and run your vehicle hourly to prevent battery discharge.
•	mportant : Turn OFF the inverter and device(s) being used before engine start up. -Regularly check that all connections are secure and tight : A loose connection can create high electrical resistance and generate excessive heat which will damage the inverter.
3.TROUBLE SHOOTING GUIDE
	Problem	CAL SE	REMEDY
	how Battery Aloe 0	denote power or ex-	Check accessory (cigarette lighter )plug and
	All the I, me	excessive voltage drop	socket connection:	lean or replace as required,
	or condition	Start	the engine recharge the Scorer-- Make
		sure inverter is turned off  before starting
		engine. replace battery if reg
	Television/power tool	I. High surge wattage re-	I toggle the ON/OFF switch in quick succession a
	will not start	quirement to start-up	total of 5 times to generate the necessary power to
		start the device if the d-, does not turn ON or
		rant up in - cycles of On OFF trials, this inverter
		will not  work with the device
	Static/Noise	5 a e	Do not use inverter with le AC filtering system
	[inference in audio sys-	n Cu... e	AC filter
	shielding	2. Replace audio system with quality noise
		filtering
	Lack or power output	I. Power source voltage	1. IRecharge vehicle battery or rupture
	below 10 volts	2.Reduce load to maximum 1000 -,s.
	being operated. 2. draw. y current	3.Turn ignition to accessory on position.
	being	ape	4.Allow inverter to cool down a minimum of 15
	3.Vehicle lighter socket	minutes before operating again.
	not working	5.Turn Off the device(s) and inverter.
	4. Thermal shutdown	Disconnect device(s) connected to inverter.Turn
	condition.	the inverter ON and leave running for a minimum
	5.Inverte not	of 2 minutes. Turn OFF inverter, quickly plug
	completely warmed up.	in device(s) to inverter making sure device(s) is
	6.Inverter fuse blown .	OFF prior to connection, turn ON the inverter
		and the device(s)
		6.Replace 40 A rated fuse. TO REPLACE FUSE;
		Locate fuse compartment in the rear of the
		inverter. Open black fuse compartment using flat
		head screw driver.Remove fuse with needle nose
		pliers and replace with spare fuse provided or
		equivalent   40 amp fuse
	Tel--on interference	1. Picture breaking up	ace the inverter, cable possible from  TV, the
	t	and coaxial cable.
		may be lit of range
	Red light On	1. Inverter is overloaded	1. Replace load to maximum of 1000	a
	2. Inverter voltage below 10 Volt	-. Charge .r replace battery.
	10 VoIt	
4.SPECIFICATION:
A.OUTPUT VOLTAGE RANGE 	220VOLT AC RMS
B.MAX.CONTINUOUS POWER 	1000 WATT
C.SURGE CAPABILITY(PEAK POWER)	2000 WATT/.01 SECOND
D.OPTIMUM EFFICIENCY 	>80%
E.NO LOAD CURRENT DRAW 	<0.9AMP
F.WAVEFORM 	MODIFIED SINE WAVE
G.INPUT VOLTAGE RANGE	11-15 VOLTS DC
H.REPLACEABLE FUSE 	40 AMP
I. AUTOMATIC ELECTRONIC CIRCUIT PROTECTION FEATURES:
a. HIGH INPUT VOLTAGE SHUTDOWN	16. 18VOLTS DC
b. LOW INPUT VOLTAGE AUDIBLE ALARM	10.5 � 0.5VOLT DC
c. LOW INPUT VOLTAGE SHUTDOWN 	10+-0.5VOLTDC
d. OVER TEMPERATURE SHUTDOWN 	150'F.
THE UNIT WILL BE AUTOMATICALLY RESTARTED AFTER APPROXIMATELY 15 MINUTES OF COOL DOWN.
e.OVERLOAD SHUTDOWN 	1050 -1200 WATT J. SYSTEM DISPLAY:
a. SYSTEM NORMAL OPERATION 	GREEN LED INDICATOR
b. OVER TEMPERATURE	RED LED INDICATOR
c. OVER LOAD 	RED LED INDICATOR
d. LOW/HIGH BATTERY	RED LED INDICATOR
K. ENVIRONMENT OPERATIONAL CONDITIONS:
OPERATING 	32 캟 TO 95 캟 L. PHYSICAL:
a. NET WEIGHT(KG.)	1.89kgs
b. DIMENSIONS 	L:266.7 x W:203.2 x H:89mm